|  |  |
| --- | --- |
| AC | alternating current |
| ADSL | asymmetric digital subscriber line |
| AR | Augmented Reality |
| ASCII | American Standard Code for Information Interchange |
| BCC | Blind CarbonCopy? |
| CC | Carbon Copy? |
| CCTV | Closed Circuit Television |
| CGI | Computer-Generated Imagery |
| CIO | Chief Information Officer/ chief investment officer |
| CO2 | Carbon dioxide |
| CPU | Central Processing Unit |
| CTO | Chief Technology Officer |
| DC | Direct Current |
| DM | Direct Message |
| ext. | Extension |
| HDMI | High-Definition Multimedia Interface |
| HTML | Hypertext Markup Language |
| ICT | Information and communication technology |
| IoT | Internet of Things |
| (O)LED | Organic Light-Emitting Diode |
| PAL | Programmable Array Logic |
| PCB | Printed circuit boards |
| PET/PETE | Polyethylene Terephthalate |
| PVC | Polyvinyl Chloride |
| QA | Quality Assurance/ quality control |
| QR code | Quick Response Code |